Skip to content

# QEMU - RetroBIOS

Type | libretro
Classification | community_fork
Source | https://github.com/io12/qemu-libretro
Upstream | https://github.com/qemu/qemu
Version | 0.1.0
Profiled | 2026-03-25
Cores | qemu
Systems | ibm-pc, x86, x86-64, ppc, ppc64, sparc, sparc64, arm, aarch64, mips, mips64, riscv32, riscv64, s390x, m68k, alpha, hppa

75 files | 2 required, 73 optional | 0 in repo, 75 missing

`SeaBIOS (128 KB)` -required, missing from repo

- Path: `qemu/bios.bin`
- Size: 128.0 KB
- SHA1: `f402170ee4f374c304a7ce0b139d6cecb1732aff`
- MD5: `e9ca30100c47a26b66488444c5b0bd15`
- Source: `hw/i386/pc_sysfw.c:222,243`
- SeaBIOS legacy BIOS for x86/x86_64 PC emulation. Default firmware loaded by pc_sysfw.c for standard PC machine types.

`SeaBIOS (256 KB)` -optional, missing from repo

- Path: `qemu/bios-256k.bin`
- Size: 256.0 KB
- SHA1: `5fe6078506094333106e6b3f33c7185dea7f0268`
- MD5: `d3dab3095c73cad67afd3cc16a88479c`
- Source: `pc-bios/meson.build:30`
- SeaBIOS 256 KB variant. Some machine types or configurations may prefer this larger image.

`SeaBIOS microvm` -optional, missing from repo

- Path: `qemu/bios-microvm.bin`
- Size: 128.0 KB
- SHA1: `56f33ced7ea0f7581d776396a0ac6cfe2c7c9257`
- MD5: `9f0ddaf6f3b213798bd414273505f2ff`
- Source: `hw/i386/microvm.c:58`
- Minimal SeaBIOS for the microvm machine type, a stripped-down x86 virtual machine with reduced device set.

`qboot ROM` -optional, missing from repo

- Path: `qemu/qboot.rom`
- Size: 16.0 KB
- SHA1: `339d3a93c967491c9f1fffe963484386f48bd22c`
- MD5: `387c48aef9497c6c2b914b1e6b9bc7aa`
- Source: `pc-bios/meson.build:32`
- Minimal x86 firmware for fast Linux kernel booting.

`VGA BIOS (ISA)` -required, missing from repo

- Path: `qemu/vgabios.bin`
- Size: 38.0 KB
- SHA1: `63d87e2a6618c3a9b2aabecf03ac2456e5e63410`
- MD5: `ecef0b49f8f4e61874f012eb12ba0e36`
- Source: `hw/display/vga-isa.c:88, hw/display/vga_int.h:191`
- Standard VGA BIOS from LGPL VGA BIOS project. Loaded by ISA VGA device (vga-isa). Default VGA for older machine types.

`VGA BIOS Cirrus` -optional, missing from repo

- Path: `qemu/vgabios-cirrus.bin`
- Size: 38.0 KB
- SHA1: `883eb2657ce29661a0466b6b41ce75411f37aad9`
- MD5: `fcd3d3c0b07a9096693d69425cd940f6`
- Source: `hw/display/cirrus_vga.c:3001, hw/display/cirrus_vga_isa.c:67`
- Cirrus Logic GD5446 VGA BIOS.

`VGA BIOS stdvga` -optional, missing from repo

- Path: `qemu/vgabios-stdvga.bin`
- Size: 38.5 KB
- SHA1: `87fbc0ecb1ee7d4d8c8c88c7d8a2fb3ec8f99ea5`
- MD5: `8117c3fd986fbbe327badfe38e77db1d`
- Source: `hw/display/vga-pci.c:387`
- Standard VGA PCI BIOS (Bochs VBE extensions).

`VGA BIOS bochs-display` -optional, missing from repo

- Path: `qemu/vgabios-bochs-display.bin`
- Size: 28.0 KB
- SHA1: `9e2edd3d835219cde63a20e2cd58107d7e96ef5b`
- MD5: `83e39bd3e056291ee50d2b5d937bab3e`
- Source: `hw/display/bochs-display.c:365`
- Bochs display device VGA BIOS.

`VGA BIOS ramfb` -optional, missing from repo

- Path: `qemu/vgabios-ramfb.bin`
- Size: 28.0 KB
- SHA1: `49df9be557f0f0277c8fedb889257e279586d536`
- MD5: `c55512e313c4cb08ec5a36198fdfef33`
- Source: `hw/display/ramfb.c:150`
- RAM framebuffer VGA BIOS.

`VGA BIOS ATI` -optional, missing from repo

- Path: `qemu/vgabios-ati.bin`
- Size: 38.5 KB
- SHA1: `ded141cacdebf557ec552597cbf57cd989cec3e2`
- MD5: `013cb287a295dc6c039921c6883a767e`
- Source: `hw/display/ati.c:1066`
- ATI VGA BIOS for emulated ATI display adapter.

`VGA BIOS QXL` -optional, missing from repo

- Path: `qemu/vgabios-qxl.bin`
- Size: 38.5 KB
- SHA1: `527227abd5f3348c382d4b02703389fbeb83b067`
- MD5: `558420a5ad839b10906d5d73e92a4160`
- Source: `hw/display/qxl.c:2512`
- QXL paravirtual display VGA BIOS.

`VGA BIOS VirtIO` -optional, missing from repo

- Path: `qemu/vgabios-virtio.bin`
- Size: 38.5 KB
- SHA1: `cddc53b94793609d1e837d78cd5468fcc1ed9164`
- MD5: `8f1e5e497342c503f62a50912f0447e0`
- Source: `hw/display/virtio-vga.c:233`
- VirtIO GPU VGA BIOS.

`VGA BIOS VMware` -optional, missing from repo

- Path: `qemu/vgabios-vmware.bin`
- Size: 38.5 KB
- SHA1: `c54901ab8f526ab201ebf1b3ecdf711e38e6c259`
- MD5: `6635fe944eab228ae01c814107674199`
- Source: `hw/display/vmware_vga.c:1349`
- VMware SVGA II display VGA BIOS.

`KVM VAPIC` -optional, missing from repo

- Path: `qemu/kvmvapic.bin`
- Size: 9.0 KB
- SHA1: `670c9cc79b4859944705eece710dc332188b79b4`
- MD5: `b8cec9572e408a3259914f9aba8664cb`
- Source: `hw/i386/vapic.c:733`
- KVM virtual APIC option ROM for APIC acceleration on x86.

`Linux boot ROM` -optional, missing from repo

- Path: `qemu/linuxboot.bin`
- Size: 1.0 KB
- SHA1: `fd19bef7f5647960952520389f448364762ed948`
- MD5: `ab40dea9ff35ec29b506fdae5bf11463`
- Source: `hw/i386/x86-common.c:964`
- Option ROM for direct Linux kernel booting via -kernel.

`Linux boot DMA ROM` -optional, missing from repo

- Path: `qemu/linuxboot_dma.bin`
- Size: 1.5 KB
- SHA1: `0bff50c10727bd9c85c831ea92b7a52699959992`
- MD5: `8cb622dc1c9290a019a801e972c9e4f9`
- Source: `hw/i386/x86-common.c:966`
- DMA-capable option ROM for direct Linux kernel booting.

`Multiboot ROM` -optional, missing from repo

- Path: `qemu/multiboot.bin`
- Size: 1.0 KB
- SHA1: `a8b58ae464fc6fb26799432ae867bf57c546ff80`
- MD5: `552a0c03c40bb3ec292f5349ea29cf86`
- Source: `hw/i386/multiboot.c:408`
- Option ROM for Multiboot kernel loading.

`Multiboot DMA ROM` -optional, missing from repo

- Path: `qemu/multiboot_dma.bin`
- Size: 1.0 KB
- SHA1: `32ab1cf336b674bfb154eb7a939a3e3275a92647`
- MD5: `e942cc4f612050c7331d33a34b0d5192`
- Source: `hw/i386/multiboot.c:406`
- DMA-capable Multiboot option ROM.

`PVH boot ROM` -optional, missing from repo

- Path: `qemu/pvh.bin`
- Size: 2.0 KB
- SHA1: `c2191e6495103c1f43e9b6ca8930e44c2245e476`
- MD5: `bb045d6f0380ad2af3531edeff92a117`
- Source: `hw/i386/x86-common.c:735`
- Option ROM for PVH (paravirtualized hardware) ELF booting.

`PXE e1000` -optional, missing from repo

- Path: `qemu/pxe-e1000.rom`
- Size: 65.5 KB
- SHA1: `368e8e9827ae8757a7449319831078b6d5efb83f`
- MD5: `898d7d0b3ed4a030c877b9185b4ef6be`
- Source: `pc-bios/meson.build:47`
- iPXE PXE boot ROM for Intel e1000 NIC (8086:100e).

`PXE eepro100` -optional, missing from repo

- Path: `qemu/pxe-eepro100.rom`
- Size: 60.0 KB
- SHA1: `b19572c9c2a11f03282df81c0397aceed409a86c`
- MD5: `2f8279177fdc2ce5abc47d9f1e303db1`
- Source: `hw/net/eepro100.c:2077`
- iPXE PXE boot ROM for Intel eepro100 NIC (8086:1209). Device default romfile.

`PXE ne2k_pci` -optional, missing from repo

- Path: `qemu/pxe-ne2k_pci.rom`
- Size: 60.0 KB
- SHA1: `f37f43f89dc99afe0442ee0b7a431ee790ad6bf6`
- MD5: `095cdf2b26084ce22adb883e9c43fc5a`
- Source: `pc-bios/meson.build:49`
- iPXE PXE boot ROM for NE2000 PCI NIC (1050:0940).

`PXE pcnet` -optional, missing from repo

- Path: `qemu/pxe-pcnet.rom`
- Size: 60.0 KB
- SHA1: `13a039bf9916f1db42d3a019591d372b4cf4aee9`
- MD5: `15e38b82922a058c6df6eaffbad1b916`
- Source: `pc-bios/meson.build:50`
- iPXE PXE boot ROM for AMD PCnet NIC (1022:2000).

`PXE rtl8139` -optional, missing from repo

- Path: `qemu/pxe-rtl8139.rom`
- Size: 60.0 KB
- SHA1: `7b512c0a7a13bc3c254a25237e4d4612170f4391`
- MD5: `22f4b6ae5650988f999ee651a3734462`
- Source: `pc-bios/meson.build:51`
- iPXE PXE boot ROM for Realtek RTL8139 NIC (10ec:8139).

`PXE virtio` -optional, missing from repo

- Path: `qemu/pxe-virtio.rom`
- Size: 59.0 KB
- SHA1: `3e3f77cfe70af904133db94f27ec24e3c9c43648`
- MD5: `91ad9770f5717a89d518534f45f1332d`
- Source: `pc-bios/meson.build:52`
- iPXE PXE boot ROM for VirtIO NIC (1af4:1000).

`EFI e1000` -optional, missing from repo

- Path: `qemu/efi-e1000.rom`
- Size: 155.5 KB
- SHA1: `a3df5fc33ab0190f470b34104ff3c0679cecbab6`
- MD5: `d8330b99643e31b51e7710fa26c7e859`
- Source: `hw/net/e1000.c:1708`
- iPXE EFI boot ROM for Intel e1000 NIC. Device default romfile.

`EFI e1000e` -optional, missing from repo

- Path: `qemu/efi-e1000e.rom`
- Size: 155.5 KB
- SHA1: `1d37f3ae6748d4deefe9fd5188a2f557bf265d61`
- MD5: `a55bf3f4988d4a736c71a1300636cd69`
- Source: `hw/net/e1000e.c:689`
- iPXE EFI boot ROM for Intel e1000e NIC. Device default romfile.

`EFI eepro100` -optional, missing from repo

- Path: `qemu/efi-eepro100.rom`
- Size: 155.5 KB
- SHA1: `956d9592fea33374ef0f1900a185b6e1109ea765`
- MD5: `d2a2f92710f5a9f77281e9492a249afb`
- Source: `pc-bios/meson.build:54`
- iPXE EFI boot ROM for Intel eepro100 NIC.

`EFI ne2k_pci` -optional, missing from repo

- Path: `qemu/efi-ne2k_pci.rom`
- Size: 154.0 KB
- SHA1: `adb7199f545fdb66c325b142c8dbc4cddb99a20d`
- MD5: `10b66275b3644af301c64a3c545c3daf`
- Source: `hw/net/ne2000-pci.c:111`
- iPXE EFI boot ROM for NE2000 PCI NIC. Device default romfile.

`EFI pcnet` -optional, missing from repo

- Path: `qemu/efi-pcnet.rom`
- Size: 154.0 KB
- SHA1: `9e5a4bb247c6a1777c89117ca091f94342b9046d`
- MD5: `374696f4fffa83c9cf18272212c21d83`
- Source: `hw/net/pcnet-pci.c:267`
- iPXE EFI boot ROM for AMD PCnet NIC. Device default romfile.

`EFI rtl8139` -optional, missing from repo

- Path: `qemu/efi-rtl8139.rom`
- Size: 157.0 KB
- SHA1: `99a1e431cc0cb0a78d5803875dfa687e12a947f4`
- MD5: `f81dbbd7001a8db631f2a548b7d08c4e`
- Source: `hw/net/rtl8139.c:3423`
- iPXE EFI boot ROM for Realtek RTL8139 NIC. Device default romfile.

`EFI virtio` -optional, missing from repo

- Path: `qemu/efi-virtio.rom`
- Size: 157.0 KB
- SHA1: `1596e9b97f0bc8b5ff3e444235690a549ee982c6`
- MD5: `d3887f04c23035cae3f0e1075deea459`
- Source: `hw/virtio/virtio-net-pci.c:73`
- iPXE EFI boot ROM for VirtIO NIC. Device default romfile.

`EFI vmxnet3` -optional, missing from repo

- Path: `qemu/efi-vmxnet3.rom`
- Size: 153.0 KB
- SHA1: `6557242402387a6319a0db6abb916ada48e1391c`
- MD5: `ea1ba222dbd5aa356ea1f29393ae55e1`
- Source: `hw/net/vmxnet3.c:2508`
- iPXE EFI boot ROM for VMware vmxnet3 NIC. Device default romfile.

`EDK2 x86_64 UEFI` -optional, missing from repo

- Path: `qemu/edk2-x86_64-code.fd`
- Size: 3.5 MB
- SHA1: `eac1a94b8e0d7c53fd5df001c36794ec34c7c724`
- Source: `pc-bios/meson.build:12`
- TianoCore UEFI firmware for x86_64. Built from edk2-stable202302.

`EDK2 x86_64 Secure Boot UEFI` -optional, missing from repo

- Path: `qemu/edk2-x86_64-secure-code.fd`
- Size: 3.5 MB
- SHA1: `617abe2746696bb4a309d72cecb446dc76a2a61e`
- Source: `pc-bios/meson.build:13`
- TianoCore UEFI firmware for x86_64 with Secure Boot support.

`EDK2 i386 UEFI` -optional, missing from repo

- Path: `qemu/edk2-i386-code.fd`
- Size: 3.5 MB
- SHA1: `45b8faebdfaaf19d16e3a7c5f60d69214685071c`
- Source: `pc-bios/meson.build:9`
- TianoCore UEFI firmware for i386.

`EDK2 i386 Secure Boot UEFI` -optional, missing from repo

- Path: `qemu/edk2-i386-secure-code.fd`
- Size: 3.5 MB
- SHA1: `6982abec8ef2ed7c8293163d5a0bd69a01a2126f`
- Source: `pc-bios/meson.build:10`
- TianoCore UEFI firmware for i386 with Secure Boot support.

`EDK2 i386 UEFI vars template` -optional, missing from repo

- Path: `qemu/edk2-i386-vars.fd`
- Size: 528.0 KB
- SHA1: `b62e676c9317a32aaa9ee1d76268d8c55663bd6e`
- Source: `pc-bios/meson.build:11`
- UEFI variable store template for i386/x86_64 EDK2 firmware.

`EDK2 AArch64 UEFI` -optional, missing from repo

- Path: `qemu/edk2-aarch64-code.fd`
- Size: 64.0 MB
- SHA1: `514edbce58bfa877170673c1799351a7dab3b6df`
- Source: `pc-bios/meson.build:4`
- TianoCore UEFI firmware for AArch64 (ARM 64-bit).

`EDK2 ARM UEFI` -optional, missing from repo

- Path: `qemu/edk2-arm-code.fd`
- Size: 64.0 MB
- SHA1: `c20f01c28b59b388abb9d0febeec45d801a632f0`
- Source: `pc-bios/meson.build:5`
- TianoCore UEFI firmware for ARM (32-bit).

`EDK2 ARM UEFI vars template` -optional, missing from repo

- Path: `qemu/edk2-arm-vars.fd`
- Size: 64.0 MB
- SHA1: `b051167e0e57bd13d77ed92ef7b474872f44ec6d`
- Source: `pc-bios/meson.build:6`
- UEFI variable store template for ARM/AArch64 EDK2 firmware.

`EDK2 RISC-V UEFI` -optional, missing from repo

- Path: `qemu/edk2-riscv-code.fd`
- Size: 32.0 MB
- SHA1: `2c8633d881ece0c4794d740138a318f7e9af480c`
- Source: `pc-bios/meson.build:7`
- TianoCore UEFI firmware for RISC-V 64-bit.

`EDK2 RISC-V UEFI vars template` -optional, missing from repo

- Path: `qemu/edk2-riscv-vars.fd`
- Size: 32.0 MB
- SHA1: `c4e6cce4247ba8f32f528c1c69f49228f616677f`
- Source: `pc-bios/meson.build:8`
- UEFI variable store template for RISC-V EDK2 firmware.

`OpenBIOS PowerPC` -optional, missing from repo

- Path: `qemu/openbios-ppc`
- Size: 661.3 KB
- SHA1: `0ef5051dcb318c0bc45d1908f8318d6eece8686a`
- Source: `hw/ppc/mac_oldworld.c:60, hw/ppc/mac_newworld.c:86`
- OpenBIOS (IEEE 1275 Open Firmware) for PowerPC emulation. Default for -M mac99, -M g3beige and other PPC machines.

`SLOF (Slimline Open Firmware)` -optional, missing from repo

- Path: `qemu/slof.bin`
- Size: 971.7 KB
- SHA1: `a03a94acfe555804d66cc6c74760ae1375a71a64`
- Source: `hw/ppc/spapr.c:106`
- IBM SLOF firmware for pSeries (POWER) machine type. Built from qemu-slof-20230918.

`skiboot` -optional, missing from repo

- Path: `qemu/skiboot.lid`
- Size: 2.4 MB
- SHA1: `8052069aa9714c23be05b4e62fb245a3d572cb0f`
- Source: `hw/ppc/pnv.c:63`
- OPAL firmware for OpenPOWER PowerNV (non-virtualized) machine type.

`VOF (Virtual Open Firmware)` -optional, missing from repo

- Path: `qemu/vof.bin`
- Size: 3.4 KB
- SHA1: `fc737b34a390f5752cb7e35b33d71f4f438ab607`
- Source: `hw/ppc/spapr.c:107, hw/ppc/pegasos2.c:43`
- Minimal Open Firmware shim for -machine pseries,x-vof=on. Also default for Pegasos II.

`VOF NVRAM` -optional, missing from repo

- Path: `qemu/vof-nvram.bin`
- Size: 16.0 KB
- SHA1: `5d1184609b87f78635f0575467a1c3f440900ff0`
- Source: `pc-bios/meson.build:83`
- NVRAM template for VOF (Virtual Open Firmware).

`U-Boot e500` -optional, missing from repo

- Path: `qemu/u-boot.e500`
- Size: 411.8 KB
- SHA1: `9ea03f249f856cdcb4399cc1f5a5031729379911`
- Source: `hw/ppc/e500.c:1184`
- U-Boot for PowerPC e500 (qemu-ppce500 target). Built from upstream denx u-boot, commit 2072e72.

`U-Boot SAM460` -optional, missing from repo

- Path: `qemu/u-boot-sam460-20100605.bin`
- Size: 512.0 KB
- SHA1: `0399a79ac0cf77f0da70af9baec7548a3b368f0a`
- Source: `pc-bios/meson.build:74`
- U-Boot for Sam460ex (AmigaOne) PowerPC board.

`QEMU VGA Mac driver` -optional, missing from repo

- Path: `qemu/qemu_vga.ndrv`
- Size: 18.3 KB
- SHA1: `638c6262a6eb579ec3d1c9292566ac94c942dc15`
- Source: `hw/ppc/mac_oldworld.c:58, hw/ppc/mac_newworld.c:84`
- QemuMacDrivers VGA driver for PPC MacOS guests.

`OpenBIOS Sparc32` -optional, missing from repo

- Path: `qemu/openbios-sparc32`
- Size: 373.1 KB
- SHA1: `5a4f2124c8f093f8aee99fbcebcf5d17d789ff26`
- Source: `hw/sparc/sun4m.c:79`
- OpenBIOS for Sparc32 emulation (sun4m).

`OpenBIOS Sparc64` -optional, missing from repo

- Path: `qemu/openbios-sparc64`
- Size: 1.5 MB
- SHA1: `c6e215fe460629d35688ab8e51faf6f765827cd6`
- Source: `hw/sparc64/sun4u.c:67`
- OpenBIOS for Sparc64 (UltraSPARC) emulation (sun4u).

`QEMU TCX display` -optional, missing from repo

- Path: `qemu/QEMU,tcx.bin`
- Size: 1.4 KB
- SHA1: `5f1792a73ee47d78b2160191ecb2c92f353f93ad`
- Source: `hw/display/tcx.c:38,827`
- TCX framebuffer FCode driver for Sparc32 OpenBIOS.

`QEMU cgthree display` -optional, missing from repo

- Path: `qemu/QEMU,cgthree.bin`
- Size: 850 B
- SHA1: `619b86fb02faf8f682474be3f0653b58015008ba`
- Source: `hw/display/cg3.c:44,303`
- CG3 framebuffer FCode driver for Sparc32 OpenBIOS.

`U-Boot LEON3` -optional, missing from repo

- Path: `qemu/u-boot.bin`
- Source: `hw/sparc/leon3.c:53`
- U-Boot for LEON3 SPARC board. Not shipped with QEMU, user-supplied.

`Alpha PALcode` -optional, missing from repo

- Path: `qemu/palcode-clipper`
- Size: 150.1 KB
- SHA1: `47b0870aaa45a7aa0d48847fd905908fb06f3e9f`
- Source: `hw/alpha/dp264.c:139`
- PALcode firmware for Alpha (Clipper/DP264) machine emulation.

`OpenSBI RISC-V 32` -optional, missing from repo

- Path: `qemu/opensbi-riscv32-generic-fw_dynamic.bin`
- Size: 262.0 KB
- SHA1: `7a23dfdeef3d78ffc89d86e89fc06a36f1e4386f`
- Source: `hw/riscv/boot.c:92`
- OpenSBI (Supervisor Binary Interface) firmware for RISC-V 32-bit.

`OpenSBI RISC-V 64` -optional, missing from repo

- Path: `qemu/opensbi-riscv64-generic-fw_dynamic.bin`
- Size: 266.1 KB
- SHA1: `6883bfd1991c0ef0d67b0967e7dcbd60420dd480`
- Source: `hw/riscv/boot.c:92`
- OpenSBI firmware for RISC-V 64-bit.

`S390 CCW firmware` -optional, missing from repo

- Path: `qemu/s390-ccw.img`
- Size: 41.6 KB
- SHA1: `7b4fa888d32ca8ddbc752f7442e4d055cee1871a`
- Source: `hw/s390x/ipl.c:149`
- Channel Command Word boot firmware for s390x emulation.

`S390 network boot` -optional, missing from repo

- Path: `qemu/s390-netboot.img`
- Size: 65.7 KB
- SHA1: `f6cec671408117bd9a31e982682662f27ef4fb2c`
- Source: `hw/s390x/ipl.c:497`
- Network boot firmware for s390x emulation.

`HP-PA firmware (32-bit)` -optional, missing from repo

- Path: `qemu/hppa-firmware.img`
- Size: 163.9 KB
- SHA1: `605c36ede6c120c6cc7efe147a75a3dc4b7e4fb0`
- Source: `hw/hppa/machine.c:424`
- SeaBIOS-hppa firmware for 32-bit HP-PARISC emulation.

`HP-PA firmware (64-bit)` -optional, missing from repo

- Path: `qemu/hppa-firmware64.img`
- Size: 201.2 KB
- SHA1: `b42f6d4ca74073de6c038579b4a9323ad0a6b398`
- Source: `hw/hppa/machine.c:424`
- SeaBIOS-hppa firmware for 64-bit HP-PARISC emulation.

`MIPS BIOS (big-endian)` -optional, missing from repo

- Path: `qemu/mips_bios.bin`
- Source: `hw/mips/malta.c:97`
- Default BIOS for big-endian MIPS machines (Malta, MIPSsim, Jazz). Not shipped with QEMU.

`MIPS BIOS (little-endian)` -optional, missing from repo

- Path: `qemu/mipsel_bios.bin`
- Source: `hw/mips/malta.c:99`
- Default BIOS for little-endian MIPS machines (Malta, MIPSsim, Jazz). Not shipped with QEMU.

`Loongson3 BIOS` -optional, missing from repo

- Path: `qemu/bios_loongson3.bin`
- Source: `hw/mips/loongson3_virt.c:63`
- Default BIOS for Loongson3 virtual MIPS machine. Not shipped with QEMU.

`PMON Fuloong2e` -optional, missing from repo

- Path: `qemu/pmon_2e.bin`
- Source: `hw/mips/fuloong2e.c:58`
- PMON monitor for Fuloong2e MIPS board. Not shipped with QEMU.

`Macintosh ROM` -optional, missing from repo

- Path: `qemu/MacROM.bin`
- Source: `hw/m68k/q800.c:62`
- Apple Macintosh ROM for Quadra 800 emulation. Not shipped with QEMU.

`Canon A1100 ROM` -optional, missing from repo

- Path: `qemu/canon-a1100-rom1.bin`
- Source: `hw/arm/digic_boards.c:131`
- Canon PowerShot A1100 IS DIGIC camera ROM. Not shipped with QEMU.

`NPCM7xx boot ROM` -optional, missing from repo

- Path: `qemu/npcm7xx_bootrom.bin`
- Size: 768 B
- SHA1: `22a75d26a0591d2c7763765b6381fa2f73de43e1`
- Source: `hw/arm/npcm7xx_boards.c:56`
- Boot ROM for Nuvoton NPCM7xx BMC (ARM Cortex-A9).

`Bamboo DTB (PPC)` -optional, missing from repo

- Path: `qemu/bamboo.dtb`
- Size: 3.1 KB
- SHA1: `ebdf1745479f4ec88459bbd9ef16ee1114018508`
- Source: `hw/ppc/ppc440_bamboo.c:38`
- Device tree blob for PowerPC Bamboo (440EP) board.

`Canyonlands DTB (PPC)` -optional, missing from repo

- Path: `qemu/canyonlands.dtb`
- Size: 9.5 KB
- SHA1: `8a2fda0b4f23a92eb44776b5d7ffe951987062da`
- Source: `hw/ppc/sam460ex.c:45`
- Device tree blob for PowerPC Canyonlands (460EX) / Sam460ex board.

`Petalogix ML605 DTB (MicroBlaze)` -optional, missing from repo

- Path: `qemu/petalogix-ml605.dtb`
- Size: 9.7 KB
- SHA1: `892d265838866869b8a8ef104252ff5b2fda156f`
- Source: `pc-bios/meson.build:91`
- Device tree blob for Xilinx Petalogix ML605 MicroBlaze board. MicroBlaze target not built in libretro core.

`Petalogix S3ADSP1800 DTB (MicroBlaze)` -optional, missing from repo

- Path: `qemu/petalogix-s3adsp1800.dtb`
- Size: 8.0 KB
- SHA1: `976600e3f89ecc1f3564b7077f53c58e0b565280`
- Source: `pc-bios/meson.build:90`
- Device tree blob for Xilinx Petalogix S3ADSP1800 MicroBlaze board. MicroBlaze target not built in libretro core.

`Virtex ML507 DTB (PPC)` -optional, missing from repo

- Path: `qemu/virtex-ml507.dtb`
- Source: `hw/ppc/virtex_ml507.c:148`
- Device tree blob for Xilinx Virtex ML507 PowerPC board. Not shipped with QEMU.

Generated on 2026-03-25T14:56:43Z