Skip to content

# FinalBurn Neo - RetroBIOS

Type | libretro
Classification | official_port
Source | https://github.com/libretro/FBNeo
Upstream | https://github.com/finalburnneo/FBNeo
Version | v1.0.0.03
Profiled | 2026-03-23
Cores | fbneo
Systems | snk-neogeo-mvs, snk-neogeo-aes, snk-neogeo-cd, snk-neogeo-pocket, capcom-cps3, igs-pgm, fairchild-channelf, coleco-colecovision, sinclair-spectrum, msx, nes-fds, super-kaneko-nova, deco-cassette, namco-na1, namco-nb1, sega-system16b, konami-bubsys, nmk16, midway-mcr, snes, taito-cchip, ym2608

Technical notes

FinalBurn Neo is a multi-system arcade and console emulator. BIOS files are expected as MAME-format ZIP archives containing individual ROM chips. The libretro core searches for BIOS ZIPs in this order (src/burner/libretro/libretro.cpp:922-1030): 1. {rom_dir}/{romName} 2. {rom_dir}/arcade/{romName} 3. {system_dir}/fbneo/{romName} 4. {system_dir}/fbneo/arcade/{romName} 5. {system_dir}/{romName}

Each game driver specifies a parent BIOS set via BurnDriver. The BIOS ZIP must contain the individual ROM chip files listed below. CRC32 values from BurnRomInfo structs are used to match ROMs inside ZIPs.

Neo Geo games reference "neogeo" as parent. The neogeo.zip BIOS set contains multiple selectable BIOS variants (MVS, AES, Universe BIOS). Only one 68K BIOS ROM is active at a time (selected via dipswitch), but the Z80 BIOS, fix tiles, and zoom table are always required.

CPS-3 games are self-contained: each game ZIP includes its own SH-2 BIOS chip. There is no shared cps3.zip. BIOS selection is per-game per-region.

PGM games reference "pgm" as parent. The pgm.zip contains shared text tiles, samples, and 68K BIOS ROMs. Some PGM sub-boards use alternate BIOS sets (theglad, dmnfrnt, svgpcb, ddp3).

Console subsystems (Channel F, ColecoVision, Spectrum, MSX, NES/FDS, NGP) each have their own BIOS set referenced as parent for their game drivers.

DECO Cassette games reference "decocass" as parent. The decocass.zip contains multiple regional BIOS variants (Japan, USA, UK, Europe) with older/newer versions for each.

144 files | 69 required, 75 optional | 7 in repo, 137 missing

`sp-s3.sp1` -required, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `91b64be3`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1604`
- MVS Asia/Europe ver. 6 (1 slot) - default BIOS

`sp-s2.sp1` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `9036d879`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1605`
- MVS Asia/Europe ver. 5 (1 slot)

`sp-s.sp1` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `c7f2fa45`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1606`
- MVS Asia/Europe ver. 3 (4 slot)

`sp-u2.sp1` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `e72943de`
- Aliases: `usa_2slt.bin`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1607`
- MVS USA ver. 5 (2 slot)

`sp1-u2` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `62f021f4`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1608`
- MVS USA ver. 5 (4 slot)

`sp-e.sp1` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `2723a5b5`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1609`
- MVS USA ver. 5 (6 slot)

`sp1-u4.bin` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `1179a30f`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1610`
- MVS USA (U4)

`sp1-u3.bin` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `2025b7a2`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1611`
- MVS USA (U3)

`vs-bios.rom` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `f0e8f27d`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1612`
- MVS Japan ver. 6

`sp-j2.sp1` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `acede59c`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1613`
- MVS Japan ver. 5

`sp1.jipan.1024` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `9fb0abe4`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1614`
- MVS Japan ver. 3 (4 slot)

`sp-45.sp1` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 512.0 KB
- CRC32: `03cc9f6a`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1615`
- NEO-MVH MV1C (Asia)

`sp-j3.sp1` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 512.0 KB
- CRC32: `486cb450`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1616`
- NEO-MVH MV1C (Japan)

`japan-j3.bin` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `dff6d41f`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1617`
- MVS Japan (J3)

`sp1-j3.bin` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `fbc6d469`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1618`
- MVS Japan (J3, alt)

`neo-po.bin` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-aes
- Size: 128.0 KB
- CRC32: `16d0c132`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1620`
- AES Japan

`neo-epo.bin` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-aes
- Size: 128.0 KB
- CRC32: `d27a71f1`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1621`
- AES Asia

`neodebug.bin` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `698ebb7d`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1622`
- Development Kit BIOS

`sp-1v1_3db8c.bin` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `162f0ebe`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1628`
- Deck ver. 6 (Git Ver 1.3)

`uni-bios_4_0.rom` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `a7aab458`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1629`
- Universe BIOS ver. 4.0 (hack)

`uni-bios_3_3.rom` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `24858466`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1630`
- Universe BIOS ver. 3.3 (hack)

`uni-bios_3_2.rom` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `a4e8b9b3`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1631`
- Universe BIOS ver. 3.2 (hack)

`uni-bios_3_1.rom` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `0c58093f`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1632`
- Universe BIOS ver. 3.1 (hack)

`uni-bios_3_0.rom` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `a97c89a9`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1633`
- Universe BIOS ver. 3.0 (hack)

`uni-bios_2_3.rom` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `27664eb5`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1634`
- Universe BIOS ver. 2.3 (hack)

`uni-bios_2_3o.rom` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `601720ae`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1635`
- Universe BIOS ver. 2.3 older (hack)

`uni-bios_2_2.rom` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `2d50996a`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1636`
- Universe BIOS ver. 2.2 (hack)

`uni-bios_2_1.rom` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `8dabf76b`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1637`
- Universe BIOS ver. 2.1 (hack)

`uni-bios_2_0.rom` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `0c12c2ad`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1638`
- Universe BIOS ver. 2.0 (hack)

`uni-bios_1_3.rom` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `b24b44a0`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1639`
- Universe BIOS ver. 1.3 (hack)

`uni-bios_1_2.rom` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `4fa698e9`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1640`
- Universe BIOS ver. 1.2 (hack)

`uni-bios_1_2o.rom` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `e19d3ce9`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1641`
- Universe BIOS ver. 1.2 older (hack)

`uni-bios_1_1.rom` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `5dda0d84`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1642`
- Universe BIOS ver. 1.1 (hack)

`uni-bios_1_0.rom` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `0ce453a0`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1643`
- Universe BIOS ver. 1.0 (hack)

`neopen.sp1` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `cb915e76`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1645`
- NeoOpen BIOS v0.1 beta (hack)

`sm1.sm1` -required, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `94416d67`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1652`
- Z80 sound BIOS

`sfix.sfix` -required, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `c2ea0cfd`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1653`
- Text layer fix tiles

`000-lo.lo` -required, in `neogeo.zip`

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `5a86cff2`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1654`
- Platforms: lakka, recalbox, retroarch, retrodeck, retropie
- Zoom lookup table

`236-bios.sp1` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `853e6b96`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1744`
- Trackball BIOS / Asia MV1B 263

`236-bios_japan_hack.sp1` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 128.0 KB
- CRC32: `02bf4426`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1745`
- Trackball BIOS / Japan (hack)

`sp-4x.sp1` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 512.0 KB
- CRC32: `b4590283`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1791`
- PCB BIOS for Metal Slug 5 PCB and SVC Chaos PCB

`spj.sp1` -optional, in `neogeo.zip`, missing from repo

- System: snk-neogeo-mvs
- Size: 512.0 KB
- CRC32: `148dd727`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1879`
- PCB BIOS for KOF 2003 PCB

`neocd.bin` -required, in `neocdz.zip`

- System: snk-neogeo-cd
- Size: 512.0 KB
- CRC32: `df9de490`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1963`
- Platforms: batocera, lakka, recalbox, retroarch, retrobat, retrodeck, retropie
- Neo Geo CD/CDZ top-loading BIOS

`neocd_sz.rom` -optional, in `neocdz.zip`

- System: snk-neogeo-cd
- Size: 512.0 KB
- CRC32: `42f6b6c4`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1964`
- Platforms: batocera, lakka, recalbox, retroarch, retrobat, retrodeck, retropie
- Neo Geo CDZ custom BIOS by SMKDan

`uni-bioscd33.rom` -optional, in `neocdz.zip`, missing from repo

- System: snk-neogeo-cd
- Size: 512.0 KB
- CRC32: `ff3abc59`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1965`
- Universe BIOS CD ver. 3.3 (hack)

`uni-bioscd32.rom` -optional, in `neocdz.zip`, missing from repo

- System: snk-neogeo-cd
- Size: 512.0 KB
- CRC32: `0ffb3127`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1966`
- Universe BIOS CD ver. 3.2 (hack)

`000-lo.lo` -required, in `neocdz.zip`

- System: snk-neogeo-cd
- Size: 128.0 KB
- CRC32: `5a86cff2`
- Source: `src/burn/drv/neogeo/d_neogeo.cpp:1968`
- Platforms: lakka, recalbox, retroarch, retrodeck, retropie
- Zoom lookup table (shared with MVS)

`pgm_t01s.rom` -required, in `pgm.zip`, missing from repo

- System: igs-pgm
- Size: 2.0 MB
- CRC32: `1a7123a0`
- Source: `src/burn/drv/pgm/d_pgm.cpp:880`
- 8x8 text layer tiles

`pgm_m01s.rom` -required, in `pgm.zip`, missing from repo

- System: igs-pgm
- Size: 2.0 MB
- CRC32: `45ae7159`
- Source: `src/burn/drv/pgm/d_pgm.cpp:881`
- ICS2115 sound samples

`pgm_p01s.u20` -optional, in `pgm.zip`, missing from repo

- System: igs-pgm
- Size: 128.0 KB
- CRC32: `e42b166e`
- Source: `src/burn/drv/pgm/d_pgm.cpp:883`
- 68K BIOS V0001 older (02/26/97)

`pgm_p02s.u20` -required, in `pgm.zip`, missing from repo

- System: igs-pgm
- Size: 128.0 KB
- CRC32: `78c15fa2`
- Source: `src/burn/drv/pgm/d_pgm.cpp:884`
- 68K BIOS V0001 newer (07/10/97)

`ddp3_bios.u37` -optional, in `pgm.zip`, missing from repo

- System: igs-pgm
- Size: 512.0 KB
- CRC32: `b3cc5c8f`
- Source: `src/burn/drv/pgm/d_pgm.cpp:886`
- 68K BIOS V0001 custom (07/17/97) for DoDonPachi III

`bios.u42` -optional, in `pgm.zip`, missing from repo

- System: igs-pgm
- Size: 128.0 KB
- CRC32: `517cf7a2`
- Source: `src/burn/drv/pgm/d_pgm.cpp:887`
- 68K BIOS V0001-01J custom (02/25/03) for The Gladiator

`svg_bios.u49` -optional, in `pgm.zip`, missing from repo

- System: igs-pgm
- Size: 128.0 KB
- CRC32: `3346401f`
- Source: `src/burn/drv/pgm/d_pgm.cpp:928`
- 68K BIOS V0001 custom (05/13/05) for SVG PCB

`sfiii_euro.29f400.u2` -required, in `sfiii.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `27699ddc`
- Source: `src/burn/drv/cps3/d_cps3.cpp:336`
- SH-2 BIOS, SF3 1st Impact Europe

`sfiii_usa_region_b1.29f400.u2` -required, in `sfiiiu.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `fb172a8e`
- Source: `src/burn/drv/cps3/d_cps3.cpp:351`
- SH-2 BIOS, SF3 1st Impact USA

`sfiii_asia_region_bd.29f400.u2` -required, in `sfiiia.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `cbd28de7`
- Source: `src/burn/drv/cps3/d_cps3.cpp:366`
- SH-2 BIOS, SF3 1st Impact Asia

`sfiii_japan.29f400.u2` -required, in `sfiiij.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `74205250`
- Source: `src/burn/drv/cps3/d_cps3.cpp:381`
- SH-2 BIOS, SF3 1st Impact Japan

`sfiii_hispanic.29f400.u2` -required, in `sfiiih.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `d2b3cd48`
- Source: `src/burn/drv/cps3/d_cps3.cpp:396`
- SH-2 BIOS, SF3 1st Impact Hispanic

`sfiii_asia_nocd.29f400.u2` -required, in `sfiiin.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `ca2b715f`
- Source: `src/burn/drv/cps3/d_cps3.cpp:411`
- SH-2 BIOS, SF3 1st Impact Asia (No CD)

`sfiii2_usa.29f400.u2` -required, in `sfiii2.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `75dd72e0`
- Source: `src/burn/drv/cps3/d_cps3.cpp:475`
- SH-2 BIOS, SF3 2nd Impact USA

`sfiii2_japan.29f400.u2` -required, in `sfiii2j.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `faea0a3e`
- Source: `src/burn/drv/cps3/d_cps3.cpp:490`
- SH-2 BIOS, SF3 2nd Impact Japan

`sfiii2_hispanic.29f400.u2` -required, in `sfiii2h.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `5c799526`
- Source: `src/burn/drv/cps3/d_cps3.cpp:505`
- SH-2 BIOS, SF3 2nd Impact Hispanic

`sfiii2_asia_nocd.29f400.u2` -required, in `sfiii2n.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `fd297c0d`
- Source: `src/burn/drv/cps3/d_cps3.cpp:520`
- SH-2 BIOS, SF3 2nd Impact Asia (No CD)

`sfiii3_euro.29f400.u2` -required, in `sfiii3.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `30bbf293`
- Source: `src/burn/drv/cps3/d_cps3.cpp:579`
- SH-2 BIOS, SF3 3rd Strike Europe

`sfiii3_usa.29f400.u2` -required, in `sfiii3u.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `ecc545c1`
- Source: `src/burn/drv/cps3/d_cps3.cpp:594`
- SH-2 BIOS, SF3 3rd Strike USA

`sfiii3_japan.29f400.u2` -required, in `sfiii3j.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `63f23d1f`
- Source: `src/burn/drv/cps3/d_cps3.cpp:609`
- SH-2 BIOS, SF3 3rd Strike Japan

`sfiii3_japan_nocd.29f400.u2` -required, in `sfiii3n.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `1edc6366`
- Source: `src/burn/drv/cps3/d_cps3.cpp:624`
- SH-2 BIOS, SF3 3rd Strike Japan (No CD)

`sfiii3_asia_nocd.29f400.u2` -required, in `sfiii3na.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `a12ebcd1`
- Source: `src/burn/drv/cps3/d_cps3.cpp:637`
- SH-2 BIOS, SF3 3rd Strike Asia (No CD)

`jojo_euro.29f400.u2` -required, in `jojo.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `513e40ec`
- Source: `src/burn/drv/cps3/d_cps3.cpp:799`
- SH-2 BIOS, JoJo's Venture Europe

`jojo_usa.29f400.u2` -required, in `jojou.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `8d40f7be`
- Source: `src/burn/drv/cps3/d_cps3.cpp:814`
- SH-2 BIOS, JoJo's Venture USA

`jojo_asia.29f400.u2` -required, in `jojoa.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `789aa72a`
- Source: `src/burn/drv/cps3/d_cps3.cpp:829`
- SH-2 BIOS, JoJo's Venture Asia

`jojo_japan.29f400.u2` -required, in `jojoj.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `02778f60`
- Source: `src/burn/drv/cps3/d_cps3.cpp:844`
- SH-2 BIOS, JoJo's Venture Japan

`jojo_asia_nocd.29f400.u2` -required, in `jojon.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `05b4f953`
- Source: `src/burn/drv/cps3/d_cps3.cpp:859`
- SH-2 BIOS, JoJo's Venture Asia (No CD)

`jojoba_euro.29f400.u2` -required, in `jojobar1.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `63cc8800`
- Source: `src/burn/drv/cps3/d_cps3.cpp:1184`
- SH-2 BIOS, JoJo's BA: Heritage Europe

`jojoba_japan.29f400.u2` -required, in `jojobajr1.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `3085478c`
- Source: `src/burn/drv/cps3/d_cps3.cpp:1199`
- SH-2 BIOS, JoJo's BA: Heritage Japan

`jojoba_euro_nocd.29f400.u2` -required, in `jojoba.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `1ee2d679`
- Source: `src/burn/drv/cps3/d_cps3.cpp:1120`
- SH-2 BIOS, JoJo's BA: Heritage Europe (No CD)

`jojoba_japan_nocd.29f400.u2` -required, in `jojoban.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `4dab19f5`
- Source: `src/burn/drv/cps3/d_cps3.cpp:1133`
- SH-2 BIOS, JoJo's BA: Heritage Japan (No CD)

`redearth_euro.29f400.u2` -required, in `redearth.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `02e0f336`
- Source: `src/burn/drv/cps3/d_cps3.cpp:1362`
- SH-2 BIOS, Red Earth Europe

`warzard_japan.29f400.u2` -required, in `warzard.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `f8e2f0c6`
- Source: `src/burn/drv/cps3/d_cps3.cpp:1377`
- SH-2 BIOS, Warzard Japan

`redearth_asia_nocd.29f400.u2` -required, in `redearthn.zip`, missing from repo

- System: capcom-cps3
- Size: 512.0 KB
- CRC32: `7a4f0851`
- Source: `src/burn/drv/cps3/d_cps3.cpp:1392`
- SH-2 BIOS, Red Earth Asia (No CD)

`sknsj1.u10` -required, in `skns.zip`, missing from repo

- System: super-kaneko-nova
- Size: 512.0 KB
- CRC32: `7e2b836c`
- Source: `src/burn/drv/pst90s/d_suprnova.cpp:1846`
- SKNS BIOS Japan

`sknse2.u10` -optional, in `skns.zip`, missing from repo

- System: super-kaneko-nova
- Size: 512.0 KB
- CRC32: `e2b9d7d1`
- Source: `src/burn/drv/pst90s/d_suprnova.cpp:1847`
- SKNS BIOS Europe

`sknsa1.u10` -optional, in `skns.zip`, missing from repo

- System: super-kaneko-nova
- Size: 512.0 KB
- CRC32: `745e5212`
- Source: `src/burn/drv/pst90s/d_suprnova.cpp:1848`
- SKNS BIOS Asia

`sknsu1.u10` -optional, in `skns.zip`, missing from repo

- System: super-kaneko-nova
- Size: 512.0 KB
- CRC32: `384d21ec`
- Source: `src/burn/drv/pst90s/d_suprnova.cpp:1849`
- SKNS BIOS USA

`sknsk1.u10` -optional, in `skns.zip`, missing from repo

- System: super-kaneko-nova
- Size: 512.0 KB
- CRC32: `ff1c9f79`
- Source: `src/burn/drv/pst90s/d_suprnova.cpp:1850`
- SKNS BIOS Korea

`sl31254.rom` -required, in `channelf.zip`, missing from repo

- System: fairchild-channelf
- Size: 1.0 KB
- CRC32: `9c047ba3`
- Source: `src/burn/drv/channelf/d_channelf.cpp:538`
- Channel F BIOS bottom half

`sl31253.rom` -required, in `channelf.zip`, missing from repo

- System: fairchild-channelf
- Size: 1.0 KB
- CRC32: `04694ed9`
- Source: `src/burn/drv/channelf/d_channelf.cpp:540`
- Channel F BIOS top half

`sl90025.rom` -optional, in `channelf.zip`, missing from repo

- System: fairchild-channelf
- Size: 1.0 KB
- CRC32: `015c1e38`
- Source: `src/burn/drv/channelf/d_channelf.cpp:541`
- Luxor Video Entertainment System BIOS (top half)

`coleco.rom` -required, in `coleco.zip`

- System: coleco-colecovision
- Size: 8.0 KB
- CRC32: `3aa93ef3`
- Source: `src/burn/drv/coleco/d_coleco.cpp:1070`
- Platforms: lakka, recalbox, retroarch, retrobat, retrodeck, retropie
- ColecoVision BIOS (Coleco, 1982)

`colecoa.rom` -optional, in `coleco.zip`, missing from repo

- System: coleco-colecovision
- Size: 8.0 KB
- CRC32: `39bb16fc`
- Source: `src/burn/drv/coleco/d_coleco.cpp:1071`
- ColecoVision BIOS thick characters (Coleco, 1982)

`svi603.rom` -optional, in `coleco.zip`, missing from repo

- System: coleco-colecovision
- Size: 8.0 KB
- CRC32: `19e91b82`
- Source: `src/burn/drv/coleco/d_coleco.cpp:1072`
- SVI-603 Coleco Game Adapter (Spectravideo, 1983)

`czz50.rom` -optional, in `coleco.zip`, missing from repo

- System: coleco-colecovision
- Size: 16.0 KB
- CRC32: `4999abc6`
- Source: `src/burn/drv/coleco/d_coleco.cpp:1073`
- Chuang Zao Zhe 50 (Bit Corporation, 1986)

`spectrum.rom` -required, in `spectrum.zip`, missing from repo

- System: sinclair-spectrum
- Size: 16.0 KB
- CRC32: `ddee531f`
- Source: `src/burn/drv/spectrum/d_spectrum.cpp:181`
- ZX Spectrum 48K BIOS

`zx128_0.rom` -required, in `spec128.zip`, missing from repo

- System: sinclair-spectrum
- Size: 16.0 KB
- CRC32: `e76799d2`
- Source: `src/burn/drv/spectrum/d_spectrum.cpp:188`
- ZX Spectrum 128K BIOS bank 0

`zx128_1.rom` -required, in `spec128.zip`, missing from repo

- System: sinclair-spectrum
- Size: 16.0 KB
- CRC32: `b96a36be`
- Source: `src/burn/drv/spectrum/d_spectrum.cpp:189`
- ZX Spectrum 128K BIOS bank 1

`zx128_2a_0.rom` -optional, in `spec1282a.zip`, missing from repo

- System: sinclair-spectrum
- Size: 16.0 KB
- CRC32: `30c9f490`
- Source: `src/burn/drv/spectrum/d_spectrum.cpp:196`
- ZX Spectrum +2A BIOS bank 0

`zx128_2a_1.rom` -optional, in `spec1282a.zip`, missing from repo

- System: sinclair-spectrum
- Size: 16.0 KB
- CRC32: `a7916b3f`
- Source: `src/burn/drv/spectrum/d_spectrum.cpp:197`
- ZX Spectrum +2A BIOS bank 1

`zx128_2a_2.rom` -optional, in `spec1282a.zip`, missing from repo

- System: sinclair-spectrum
- Size: 16.0 KB
- CRC32: `c9a0b748`
- Source: `src/burn/drv/spectrum/d_spectrum.cpp:198`
- ZX Spectrum +2A BIOS bank 2

`zx128_2a_3.rom` -optional, in `spec1282a.zip`, missing from repo

- System: sinclair-spectrum
- Size: 16.0 KB
- CRC32: `b88fd6e3`
- Source: `src/burn/drv/spectrum/d_spectrum.cpp:199`
- ZX Spectrum +2A BIOS bank 3

`msx.rom` -required, in `msx.zip`, missing from repo

- System: msx
- Size: 32.0 KB
- CRC32: `a317e6b4`
- Source: `src/burn/drv/msx/d_msx.cpp:1773`
- MSX1 standard BIOS

`msxj.rom` -optional, in `msx.zip`, missing from repo

- System: msx
- Size: 32.0 KB
- CRC32: `071135e0`
- Source: `src/burn/drv/msx/d_msx.cpp:1774`
- MSX1 Japanese BIOS

`kanji.rom` -optional, in `msx.zip`, missing from repo

- System: msx
- Size: 256.0 KB
- CRC32: `1f6406fb`
- Source: `src/burn/drv/msx/d_msx.cpp:1775`
- MSX Kanji character support

`fdsbios.nes` -required, in `fdsbios.zip`, missing from repo

- System: nes-fds
- Size: 8.0 KB
- CRC32: `5e607dcf`
- Source: `src/burn/drv/nes/d_nes.cpp:517`
- Famicom Disk System BIOS

`SNK Neo-Geo Pocket BIOS (1998)(SNK)(en-ja).bin` -required, in `ngp.zip`, missing from repo

- System: snk-neogeo-pocket
- Size: 64.0 KB
- CRC32: `6232df8d`
- Source: `src/burn/drv/pst90s/d_ngp.cpp:962`
- Neo Geo Pocket (b&w) BIOS

`SNK Neo-Geo Pocket Color BIOS (1999)(SNK)(en-ja).bin` -required, in `ngp.zip`, missing from repo

- System: snk-neogeo-pocket
- Size: 64.0 KB
- CRC32: `6eeb6f40`
- Source: `src/burn/drv/pst90s/d_ngp.cpp:963`
- Neo Geo Pocket Color BIOS

`v0a-.7e` -required, in `decocass.zip`, missing from repo

- System: deco-cassette
- Size: 4.0 KB
- CRC32: `3d33ac34`
- Source: `src/burn/drv/dataeast/d_decocass.cpp:3596`
- BIOS A Japan, Main M6502

`v1-.5a` -required, in `decocass.zip`, missing from repo

- System: deco-cassette
- Size: 2.0 KB
- CRC32: `b66b2c2a`
- Source: `src/burn/drv/dataeast/d_decocass.cpp:3599`
- BIOS A Japan, Sound M6502 (shared across regions)

`v2.3m` -optional, in `decocass.zip`, missing from repo

- System: deco-cassette
- Size: 32 B
- CRC32: `238fdb40`
- Source: `src/burn/drv/dataeast/d_decocass.cpp:3601`
- BIOS PROM (shared across regions)

`v4.10d` -optional, in `decocass.zip`, missing from repo

- System: deco-cassette
- Size: 32 B
- CRC32: `3b5836b4`
- Source: `src/burn/drv/dataeast/d_decocass.cpp:3602`
- BIOS PROM (shared across regions)

`v3.3j` -optional, in `decocass.zip`, missing from repo

- System: deco-cassette
- Size: 32 B
- CRC32: `51eef657`
- Source: `src/burn/drv/dataeast/d_decocass.cpp:3603`
- BIOS PROM (shared across regions)

`dsp-3_p0-a.m9` -optional, in `decocass.zip`, missing from repo

- System: deco-cassette
- Size: 2.0 KB
- CRC32: `2541e34b`
- Source: `src/burn/drv/dataeast/d_decocass.cpp:3608`
- BIOS A Japan Older, Main M6502 (part 1)

`dsp-3_p1-.l9` -optional, in `decocass.zip`, missing from repo

- System: deco-cassette
- Size: 2.0 KB
- CRC32: `3bfff5f3`
- Source: `src/burn/drv/dataeast/d_decocass.cpp:3609`
- BIOS A Japan Older, Main M6502 (part 2, shared)

`rms-3_p2-.c9` -optional, in `decocass.zip`, missing from repo

- System: deco-cassette
- Size: 1.0 KB
- CRC32: `6c4a891f`
- Source: `src/burn/drv/dataeast/d_decocass.cpp:3611`
- BIOS A Japan Older, Sound M6502 (shared)

`dsp-3_p3-.e5` -optional, in `decocass.zip`, missing from repo

- System: deco-cassette
- Size: 32 B
- CRC32: `539a5a64`
- Source: `src/burn/drv/dataeast/d_decocass.cpp:3613`
- BIOS Older PROM (shared)

`rms-3_p4-.f6` -optional, in `decocass.zip`, missing from repo

- System: deco-cassette
- Size: 32 B
- CRC32: `9014c0fd`
- Source: `src/burn/drv/dataeast/d_decocass.cpp:3614`
- BIOS Older PROM (shared)

`dsp-3_p5-.m4` -optional, in `decocass.zip`, missing from repo

- System: deco-cassette
- Size: 32 B
- CRC32: `e52089a0`
- Source: `src/burn/drv/dataeast/d_decocass.cpp:3615`
- BIOS Older PROM (shared)

`v0b-.7e` -optional, in `decocass.zip`, missing from repo

- System: deco-cassette
- Size: 4.0 KB
- CRC32: `23d929b7`
- Source: `src/burn/drv/dataeast/d_decocass.cpp:3620`
- BIOS B USA, Main M6502

`dsp-3_p0-b.m9` -optional, in `decocass.zip`, missing from repo

- System: deco-cassette
- Size: 2.0 KB
- CRC32: `b67a91d9`
- Source: `src/burn/drv/dataeast/d_decocass.cpp:3632`
- BIOS B USA Older, Main M6502

`v0c-.7e` -optional, in `decocass.zip`, missing from repo

- System: deco-cassette
- Size: 4.0 KB
- CRC32: `9f505709`
- Source: `src/burn/drv/dataeast/d_decocass.cpp:3644`
- BIOS C UK, Main M6502

`dsp-3_p0-c.m9` -optional, in `decocass.zip`, missing from repo

- System: deco-cassette
- Size: 2.0 KB
- CRC32: `c76c4057`
- Source: `src/burn/drv/dataeast/d_decocass.cpp:3656`
- BIOS C UK Older, Main M6502

`v0d-.7e` -optional, in `decocass.zip`, missing from repo

- System: deco-cassette
- Size: 4.0 KB
- CRC32: `1e0c22b1`
- Source: `src/burn/drv/dataeast/d_decocass.cpp:3668`
- BIOS D Europe, Main M6502

`dsp-3_p0-d.m9` -optional, in `decocass.zip`, missing from repo

- System: deco-cassette
- Size: 2.0 KB
- CRC32: `4b7d72bc`
- Source: `src/burn/drv/dataeast/d_decocass.cpp:3680`
- BIOS D Europe Older, Main M6502

`cassmcu.1c` -required, in `decocass.zip`, missing from repo

- System: deco-cassette
- Size: 1.0 KB
- CRC32: `a6df18fd`
- Source: `src/burn/drv/dataeast/d_decocass.cpp:3692`
- MCU BIOS, shared across all DECO Cassette regions

`c69.bin` -required, in `namcoc69.zip`, missing from repo

- System: namco-na1
- Size: 16.0 KB
- CRC32: `349134d9`
- Source: `src/burn/drv/pst90s/d_namcona1.cpp:1346`
- C69 MCU internal ROM for Namco NA-1

`c70.bin` -required, in `namcoc70.zip`, missing from repo

- System: namco-na1
- Size: 16.0 KB
- CRC32: `b4015f23`
- Source: `src/burn/drv/pst90s/d_namcona1.cpp:1367`
- C70 MCU internal ROM for Namco NA-2

`c75.bin` -required, in `namcoc75.zip`, missing from repo

- System: namco-nb1
- Size: 16.0 KB
- CRC32: `42f539a5`
- Source: `src/burn/drv/pst90s/d_namconb1.cpp:1978`
- C75 MCU internal ROM for Namco NB-1

`boot.bin` -required, in `bubsys.zip`

- System: konami-bubsys
- Size: 480 B
- CRC32: `f0774fc2`
- Source: `src/burn/drv/konami/d_nemesis.cpp:4526`
- Platforms: lakka, retroarch, retropie
- M68000 vectors

`400b03.8g` -required, in `bubsys.zip`, missing from repo

- System: konami-bubsys
- Size: 8.0 KB
- CRC32: `85c2afc5`
- Source: `src/burn/drv/konami/d_nemesis.cpp:4530`
- Z80 code

`400a1.2b` -required, in `bubsys.zip`, missing from repo

- System: konami-bubsys
- Size: 256 B
- CRC32: `5827b1e8`
- Source: `src/burn/drv/konami/d_nemesis.cpp:4532`
- K005289 wavetable 1

`400a2.1b` -required, in `bubsys.zip`, missing from repo

- System: konami-bubsys
- Size: 256 B
- CRC32: `2f44f970`
- Source: `src/burn/drv/konami/d_nemesis.cpp:4533`
- K005289 wavetable 2

`ism2006v00.u1` -required, in `isgsm.zip`, missing from repo

- System: sega-system16b
- Size: 128.0 KB
- CRC32: `2292585c`
- Source: `src/burn/drv/sega/d_sys16b.cpp:11045`
- ISG Selection Master Type 2006 BIOS

`nmk004.bin` -required, in `nmk004.zip`, missing from repo

- System: nmk16
- Size: 8.0 KB
- CRC32: `8ae61a09`
- Source: `src/burn/drv/pst90s/d_nmk16.cpp:6123`
- NMK004 TLCS90 internal ROM

`cchip_upd78c11.bin` -required, in `cchip.zip`, missing from repo

- System: taito-cchip
- Size: 4.0 KB
- CRC32: `43021521`
- Source: `src/burn/drv/taito/d_taitof2.cpp:4392`
- Taito C-Chip UPD78C11 internal ROM

`82s123.12d` -required, in `midssio.zip`, missing from repo

- System: midway-mcr
- Size: 32 B
- CRC32: `e1281ee9`
- Source: `src/burn/drv/pre90s/d_mcr.cpp:1629`
- Midway SSIO sound PROM

`ym2608_adpcm_rom.bin` -required, in `ym2608.zip`, missing from repo

- System: ym2608
- Size: 8.0 KB
- CRC32: `23c9e0d8`
- Source: `src/burn/drv/pst90s/d_pipedrm.cpp:876`
- YM2608 internal ADPCM-A rhythm samples, used by multiple drivers

`st010.bin` -required, in `st010.zip`, missing from repo

- System: snes
- Size: 68.0 KB
- CRC32: `aa11ee2d`
- Source: `src/burn/drv/snes/d_snes.cpp:571`
- Seta ST010 coprocessor microcode

`st011.bin` -required, in `st011.zip`, missing from repo

- System: snes
- Size: 68.0 KB
- CRC32: `34d2952c`
- Source: `src/burn/drv/snes/d_snes.cpp:590`
- Seta ST011 coprocessor microcode

`dsp1.bin` -required, in `dsp1.zip`, missing from repo

- System: snes
- Size: 10.0 KB
- CRC32: `2838f9f5`
- Source: `src/burn/drv/snes/d_snes.cpp:610`
- DSP-1 coprocessor microcode

`dsp1b.bin` -required, in `dsp1b.zip`, missing from repo

- System: snes
- Size: 10.0 KB
- CRC32: `453557e0`
- Source: `src/burn/drv/snes/d_snes.cpp:629`
- DSP-1B coprocessor microcode (revised)

`dsp2.bin` -required, in `dsp2.zip`, missing from repo

- System: snes
- Size: 10.0 KB
- CRC32: `8e9fbd9b`
- Source: `src/burn/drv/snes/d_snes.cpp:648`
- DSP-2 coprocessor microcode

`dsp3.bin` -required, in `dsp3.zip`, missing from repo

- System: snes
- Size: 10.0 KB
- CRC32: `6b86728a`
- Source: `src/burn/drv/snes/d_snes.cpp:667`
- DSP-3 coprocessor microcode

`dsp4.bin` -required, in `dsp4.zip`, missing from repo

- System: snes
- Size: 10.0 KB
- CRC32: `ce0c7783`
- Source: `src/burn/drv/snes/d_snes.cpp:686`
- DSP-4 coprocessor microcode

`hiscore.dat` -optional

- Path: `fbneo/hiscore.dat`
- Source: `src/burn/hiscore.cpp:406`
- High score database, enables persistent high scores across all arcade games

Generated on 2026-03-25T14:56:43Z